{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Accueil","official channels","lower Channels","lower B channels","upper D channels","upper E channels"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Accueil","index":0,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
["Bienvenue"]

{"sheet":"official channels","index":1,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Cannaux Officiels"]
["Channel","FREQUENCY (MHz)","Channel2","FREQUENCY (MHz)2"]
[1,26.965,21,27.215]
[2,26.975000000000001,22,27.225000000000001]
[3,26.984999999999999,23,27.254999999999999]
[4,27.004999999999999,24,27.234999999999999]
[5,27.015000000000001,25,27.245000000000001]
[6,27.024999999999999,26,27.265000000000001]
[7,27.035,27,27.274999999999999]
[8,27.055,28,27.285]
[9,27.065000000000001,29,27.295000000000002]
[10,27.074999999999999,30,27.305]
[11,27.085000000000001,31,27.315000000000001]
[12,27.105,32,27.324999999999999]
[13,27.114999999999998,33,27.335000000000001]
[14,27.125,34,27.344999999999999]
[15,27.135000000000002,35,27.355]
[16,27.155000000000001,36,27.364999999999998]
[17,27.164999999999999,37,27.375]
[18,27.175000000000001,38,27.385000000000002]
[19,27.184999999999999,39,27.395]
[20,27.204999999999998,40,27.405000000000001]

{"sheet":"lower Channels","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux inférieurs A"]
["Channel","Fréquency(MHz)","Channel2","Fréquency (MHz)2"]
[1,26.065000000000001,21,26.315000000000001]
[2,26.074999999999999,22,26.324999999999999]
[3,26.085000000000001,23,26.355]
[4,26.105,24,26.335000000000001]
[5,26.114999999999998,25,26.344999999999999]
[6,26.125,26,26.364999999999998]
[7,26.135000000000002,27,26.375]
[8,26.155000000000001,28,26.385000000000002]
[9,26.164999999999999,29,26.395]
[10,26.175000000000001,30,26.405000000000001]
[11,26.184999999999999,31,26.414999999999999]
[12,26.204999999999998,32,26.425000000000001]
[13,26.215,33,26.434999999999999]
[14,26.254999999999999,34,26.445]
[15,26.234999999999999,35,26.454999999999998]
[16,26.254999999999999,36,26.465]
[17,26.265000000000001,37,26.475000000000001]
[18,26.274999999999999,38,26.484999999999999]
[19,26.285,39,26.495000000000001]
[20,26.305,40,26.504999999999999]

{"sheet":"lower B channels","index":3,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux inférieurs B"]
["Channel","Fréquency (MHz)","Channel2","Fréquency (MHz)2","Fréquency (MHz)3"]
[1,26.515000000000001,21,26.765000000000001]
[2,26.524999999999999,22,26.774999999999999]
[3,26.535,23,26.785]
[4,26.555,24,26.795000000000002]
[5,26.565000000000001,25,26.805]
[6,26.574999999999999,26,26.815000000000001]
[7,26.585000000000001,27,26.824999999999999]
[8,26.605,28,26.835000000000001]
[9,26.515000000000001,29,26.844999999999999]
[10,26.625,30,26.855]
[11,26.635000000000002,31,26.864999999999998]
[12,26.655000000000001,32,26.875]
[13,26.664999999999999,33,26.885000000000002]
[14,26.675000000000001,34,26.895]
[15,26.684999999999999,35,26.905000000000001]
[16,26.704999999999998,36,26.914999999999999]
[17,26.715,37,26.925000000000001]
[18,26.725000000000001,38,26.934999999999999]
[19,26.734999999999999,39,26.945]
[20,26.754999999999999,40,26.954999999999998]

{"sheet":"upper D channels","index":4,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux supérieurs  D"]
["Channel","Fréquency (MHz)","Channel2","Fréquency (MHz)2"]
[1,27.414999999999999,21,27.664999999999999]
[2,27.425000000000001,22,27.675000000000001]
[3,27.434999999999999,23,27.704999999999998]
[4,27.454999999999998,24,27.684999999999999]
[5,27.465,25,27.695]
[6,27.475000000000001,26,27.715]
[7,27.484999999999999,27,27.725000000000001]
[8,27.504999999999999,28,27.734999999999999]
[9,27.515000000000001,29,27.745000000000001]
[10,27.524999999999999,30,27.754999999999999]
[11,27.535,31,27.765000000000001]
[12,27.555,32,27.774999999999999]
[13,27.565000000000001,33,27.785]
[14,27.574999999999999,34,27.795000000000002]
[15,27.585000000000001,35,27.805]
[16,27.605,36,27.815000000000001]
[17,27.614999999999998,37,27.824999999999999]
[18,27.625,38,27.835000000000001]
[19,27.635000000000002,39,27.844999999999999]
[20,27.655000000000001,40,27.855]

{"sheet":"upper E channels","index":5,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux Supérieurs E"]
["Channel","Fréquency (MHz)","Channel2","Fréquency(MHz)2"]
[1,27.864999999999998]
[2,27.675000000000001]
[3,27.885000000000002]
[4,27.905000000000001]
[5,27.914999999999999]
[6,27.925000000000001]
[7,27.934999999999999]
[8,27.954999999999998]
[9,27.965]
[10,27.975000000000001]
[11,27.984999999999999]